ABSTRACT
 
Ministry of Health ofRepublic of Indonesia 
Polytechnic of Health Yogyakarta 
Environmental health Departmen
 Scientific Paper, 2010
 
YAHYA ARIF HIDAYAT
 
Influence of  Various Type of Drier Pallet at Method SODIS (Solar Watter Disinfection) To E.Coli Irrigate The Well Dig The Orchard Kenteng, Nogotirto, Gamping, Sleman 
(xii + 37 pages + x attachments)

Background: Solar Water Disinfection ( SODIS) represent one of alternative of processing drinking water by exploiting sunshine. To lessen the negative impact  effect  consume the under the way water hence we can conducted by processing with the method SODIS. A lot of matter which can influence the this technology SODIS, one of them is drier pallet.
 
Research Target: To know the influence of pallet type, hence require to be conducted by research of type of drier pallet capable to degrade the E.Coli better.
 
Research Method: This Research represent the type of research of experiment pre by design is research of One Group Pre test-Post test the Control Design. This Research is done  to know the influence of various pallet of zinc drier, metal tile and almunium in degrading rate E.Coli irrigate the well dig. This research is done with the inspection E.Coli in laboratory. Data result of inspection analysed descriptively and statistical with the test of later one way anova continued with the test LSD use the SPSS 13,0 program of for windows with the belief storey;level 95% or = 0,05.
 
Result of: Research address the mean of degradation E.Coli of zinc pallet 97,61 %, metal tile pallet 68,56 % and almunium 88,01 %. After the data analysed with the test of one way anova got result P-Value 0,380, hence from the result indicated that third pallet type own the potency which is in degrading E.Coli which proved with there no difference which signifikan statistically among the treatment. Result LSD known by there no difference of degradation E.Coli which signifikan usher the treatment group.

Conclusion: descriptively is became of  the highest degradation of zinc pallet with the degradation mean 97,61 % so that zinc pallet represent the most effective pallet in degrading E.Coli irrigate the well dig at process SODIS.
 
Key word 	: Sodis, Drier Pallet, Degradation of E.Coli

Bibliography : 18 pieces (1992-2010)